**Summary of Speed Indicator Device (SID) Activity**

**For the Period 5th December 2020 to 10th January 2021**

**Location :** During this period the SID was positioned on the Stratford Tony Road at the West end of the village, which is in a 40 mph speed limit zone.The SID was mounted on a relocatable post on the left-hand side of the road as you enter Coombe Bissett village coming from the direction of Stratford Tony. This site is currently the only approved site on the Stratford Tony road.

For further information regarding approved SID sites in Coombe Bissett and Homington villages please refer to the SID location Power Point guide.

**Detailed PDF reports:**

Please refer to the tab for Stratford Tony Road for more detailed analysis of traffic data recorded by the SID, which is presented in PDF report format. Guidance Notes to each section of the PDF reports are provided below this summary.

Note: Our SID does not have GPS and therefore its reports are location agnostic. References in reports to Incoming and Outgoing traffic refer to traffic coming towards the device (Incoming) and traffic going past the device in the opposite direction (Outgoing).

**Period 5th to 17th December 2020**

Location: Stratford Tony Road, 40 mph speed limit zone. The SID was facing traffic ***coming into*** the village.

|  |  |  |
| --- | --- | --- |
| **Traffic vs. SID** | Towards | Away |
| **Traffic in relation to the village** | Incoming | Outgoing |
| Average Speed (mph) | 32.86 | 35.5 |
| Maximum Speed (mph) | 57.00 | 71.00 |
| Traffic Volume (# vehicles) | 19,135 | 17,028 |
| % Less than 46 mph\* | 99.51 | 96.11 |
| 85th %ile Speed (mph) | 37.00 | 40.00 |

\*Police enforcement in a 40 mph limit is liable at speeds > 46 mph

**Period 25th December 2020 to 10th January 2021**

Location: Stratford Tony Road, 40 mph speed limit zone. The SID was facing traffic ***leaving*** the village.

|  |  |  |
| --- | --- | --- |
| **Traffic vs. SID** | Towards | Away |
| **Traffic in relation to the village** | Outgoing | Incoming |
| Average Speed (mph) | 33.65 | 35.45 |
| Maximum Speed (mph) | 72.00 | 103.00 |
| Traffic Volume (# vehicles) | 13,155 | 14,939 |
| % Less than 46 mph\* | 97.64 | 96.82 |
| 85th %ile Speed (mph) | 38.00 | 40.00 |

\* Police enforcement in a 40 mph limit is liable at speeds > 46 mph

The Coombe Bissett Community Speed Watch (CSW) managed to hold one session on 17th December during a week that was affected by poor weather. CSW activity was subsequently suspended again on 4th January 2021 and remains so for the duration of the current Lockdown.