**Summary of Speed Indicator Device (SID) Activity**

**For the Period 24th June to 21st July 2021**

**Location :** During this period the SID was positioned on the Stratford Tony Road at the West end of the village, which is in a 40 mph speed limit zone.The SID was mounted on a relocatable post on the left-hand side of the road as you enter Coombe Bissett village coming from the direction of Stratford Tony. This site is currently the only approved site on the Stratford Tony road.

For further information regarding approved SID sites in Coombe Bissett and Homington villages please refer to the SID location Power Point guide.

**Detailed PDF reports:**

Please refer to the tab for Stratford Tony Road for more detailed analysis of traffic data recorded by the SID, which is presented in PDF report format. Guidance Notes to each section of the PDF reports are provided below this summary.

Note: Our SID does not have GPS and therefore its reports are location agnostic. References in reports to Incoming and Outgoing traffic refer to traffic coming towards the device (Incoming) and traffic going past the device in the opposite direction (Outgoing).

**Period 24th June to 4th July 2021**

Location: Stratford Tony Road, 40 mph speed limit zone. The SID was facing traffic ***coming into*** the village.

|  |  |  |
| --- | --- | --- |
| **Traffic vs. SID** | Towards | Away |
| **Traffic in relation to the village** | Incoming  | Outgoing  |
| Average Speed (mph) | 32.77 | 35.11 |
| Maximum Speed (mph) | 58.00 | 74.00 |
| Traffic Volume (# vehicles) | 20,350 | 17,458 |
| % Less than 46 mph\*  | 99.00 | 96.35 |
| 85th %ile Speed (mph) | 37.00 | 40.00 |

\*Police enforcement in a 40 mph limit is liable at speeds > 46 mph

**Period 10th July to 21st July 2021**

Location: Stratford Tony Road, 40 mph speed limit zone. The SID was facing traffic ***leaving*** the village.

|  |  |  |
| --- | --- | --- |
| **Traffic vs. SID** | Towards | Away |
| **Traffic in relation to the village** | Outgoing  | Incoming  |
| Average Speed (mph) | 33.72 | 34.67 |
| Maximum Speed (mph) | 75.00 | 94.00 |
| Traffic Volume (# vehicles) | 17,616 | 19,746 |
| % Less than 46 mph\*  | 97.74 | 97.73 |
| 85th %ile Speed (mph) | 38.00 | 39.00 |

\* Police enforcement in a 40 mph limit is liable at speeds > 46 mph

Traffic speeds remain within tolerable limits at this location. There is little variation with data gathered the last time the SID was at this location between 5th December 2020 and 10th January 2021.

The Coombe Bissett Community Speed Watch (CSW) was active during the months of June and July. Sessions were held at Tottens Farm (23rd, 30th June, 20th July), Hunter’s Lodge (1st July) and Deegan House 2nd, 22nd July). A total of 2,404 vehicles were monitored over 6 sessions of which 114 were reported to CSW Trowbridge for speeding. 25 of these drivers were speeding excessively despite the presence of up to 3 team members standing on the side of the road in Hi-Viz jackets. We have ensured to notify PC Mark Douglas and his team of all our planned CSW sessions and we are pleased to report that he supported the team at a CSW session held on 1st September. A full report will be provided in the next update.